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Laboratory task 6: Hardening medium inspection



	


Name and Surname: 



Assignment: For the specified hardening oil, make the necessary measurements to obtain the cooling curve and other parameters specified in the appendix. Measure for temperatures: RT, 50°C and 70°C. Fill in the table according to the obtained values. Briefly characterize the specified oil. 
Oil designation – test designation – testing temperature – up to – cooling time in seconds – cooling rate CR - 
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Designation of oil
Designation of test
Testing temperature
Cooling time in seconds
Up to
Cooling speed CR
Temperature
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Označení oleje 
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Čas ochlazování v sec



Označení testu



Testovací teplota
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