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Laboratory task 2: Heat treatment of the assigned steel
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Name and Surname: 




1. Carry out the heat treatment of steel …… .. according to the specified requirements (normalization annealing, soft annealing, hardening, hardening + tempering …… °C). It will always be specified for an individual task 
a. Carry out in lab TZ – UU006
2. Evaluate the relevant microstructures and assign them to the TZ mode.
3. Carry out a hardness measurement according to HRC, possibly HBW.
4. Conclusion
a. Here show a graph of TZ (temperature - approximately - of the surface, cores and furnaces), cooling environment. What structure and hardness was achieved by this TZ. 
Ing. Jiří Hájek, Ph.D.
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